**Ohio**

|  |  |
| --- | --- |
| What must be recorded/documented | Chlorine, pH, water temperature, water clarity, Cyanuric Acid, Total Alkalinity |
| Water Testing Frequency | The disinfectant residual shall be tested daily at the poolside deck prior to bathers entering the public swimming pool and every four hours when the public swimming pool is open for use. The disinfectant residual for a public swimming pool where an automatic chemical controller is installed shall be tested daily at the pool deck prior to bathers entering the water and every twelve hours the public swimming pool is open for use. (ii) Combined chlorine shall be tested daily prior to bathers entering the public swimming pool and every four hours the public swimming pool is open for use;  pH shall be tested daily prior to bathers entering the public swimming pool and every four hours when the public swimming pool is open for use. A manual test for pH shall be performed at the spray nozzles on at least one special feature every six hours when the public swimming pool is open for use;  Water temperature shall be recorded not less than once per day;  Water clarity shall be assessed continuously while the public swimming pool is in use and any problem with clarity shall be recorded as it occurs;  Total alkalinity shall be tested not less than once per week;  Cyanuric acid shall be tested not less than once per week; |
| Chlorine Levels (minimums) | POOL:  1.0  SPA: 2.0 |
| pH Levels (Min-Max) | 7.2-7.8 |
| Total Alkalinity | 60 or above |
| Max. Temperature | 90 for pools; 104 for spas |
| Spa Water Replacement | At least once every 30 days |
| Chlorine Test Kit Requirements | DPD |
| pH Test Kit Requirements | No standard |
| Cyanuric Acid Levels (Min-Max) | Max of 70 ppm |
| Water Clarity | the deepest point of the swimming pool is readily visible when viewed from the deck. |
| Turnover Rate | POOL: 8 hrs. SPA: 30 minutes WADING: 2 hrs. |
| Bather Load (per bather) | **POOL**: not specified **SPA:** not specified **WADING**: not specified |
| Depth Markings | The depth of water at a public swimming pool shall be marked at:  (a) Maximum and minimum points; and  (b) The points of break between the deep and shallow portions of a public swimming pool and at intermediate points.  Deck markers shall not be spaced more than twenty-five feet apart as measured along the perimeter wall of a public swimming pool and shall be placed:  (a) On top of the deck; and  (b) Within two feet of the water's edge or within six inches of the back of the gutter;  Depth markers shall reflect the water depth to the nearest six inch or one-half foot increment.  Depth marking numerals shall be plainly marked, at least four inches in size and of a color that contrasts with the background.  The units of measure to denote the water depth shall be spelled out in feet and inches and may be abbreviated as: ft or in.  A minimum of two depth markings per public spa, wading pool or zero entry pool shall be provided. |
| Phone | Within 500 feet of the pool |
| CPO® Required | No |