**West Virginia**

|  |  |
| --- | --- |
| What must be recorded/documented | Chlorine/Bromine, pH, Total Alkalinity |
| Water Testing Frequency | At least twice daily |
| Chlorine Levels (Min-Max) | POOL:  1.0-5.0 CL, 2.0-5.0 BRSPA: 1.0-5.0 CL, 2.0-5.0 BRWADING: 1.0-5.0 CL, 2.0-5.0 BR |
| pH Levels (Min-Max) | 7.2-7.8 |
| Chlorine Test Kit Requirements | DPD |
| pH Test Kit Requirements | No standard |
| Cyanuric Acid Levels (Min-Max) | 10-100 ppm |
| Water Clarity | 6″ black disk visible at deepest point |
| Turnover Rate | POOL: 6 hrsSPA: 30 minutesWADING: 2-4  hrs |
| Bather Load (per bather) | **POOL**: not specified**SPA:** not specified**WADING**: not specified |
| Depth Markings | Not specified |
| Total Alkalinity | 60-180 ppm |
| CPO® Required | YES |